{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Sheet1","Sheet4","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"merged":[[0,0,0,7],[1,0,1,7],[2,1,2,2],[3,0,6,0],[3,1,6,1],[7,0,10,0],[7,1,10,1],[12,0,13,0],[12,1,13,1],[15,0,16,0],[15,1,16,1],[22,0,22,7]],"flags":["formulas_cached_only"]}
["附件：采购需求表"]
["2022年广东江门国家农业科技园区核心区农业设施维修维护项目-温室大棚维修项目"]
["序号","材 料 名 称",null,"规    格","单位","数量","单价","金额"]
[1,"温室E","山墙薄膜更换","0.13mm,80m*3.3m","幅",2]
[null,null,"天面薄膜更换","0.13mm,52.5m*9.5m","幅",3]
[null,null,"侧墙薄膜更换","0.13mm,52.5m*3.5m","幅",2]
[null,null,"卡簧","包塑，2m/条","条",650]
[2,"温室H","天面检修补漏","水槽、薄膜孔洞补漏","㎡",4800]
[null,null,"主构拉筋调整","拆除垫高重新安装","项",1]
[null,null,"水帘检修补漏","水帘水槽补漏","项",1]
[null,null,"内遮阳维修","牵引材维修，驱动系统检修","㎡",4800]
[3,"温室D1","玻璃更换","5mm玻璃，735mm*1650mm","块",1]
[4,"温室D2","更换遮阳电机","专用电机，自带行程开关","个",1]
[null,null,"外遮阳检修","遮阳网、支撑线、钢丝绳、固定圈检查并更换损坏部分","㎡",188]
[5,"温室D3","外遮阳检修","遮阳网、支撑线、钢丝绳、固定圈检查，并更换损坏部分","㎡",188]
[6,"温室D4","更换侧窗电机","专用电机，自带行程开关","台",2]
[null,null,"外遮阳检修","遮阳网、支撑线、钢丝绳、固定圈检查，并更换损坏部分，更换1条牵引型材","㎡",188]
[7,"温室A","外遮阳检修","遮阳网、支撑线、钢丝绳、固定圈检查并更换损坏部分，更换一条卷轴及3条牵引型材","㎡",1536]
[8,"9号温室","外遮阳检修","遮阳网、支撑线、钢丝绳、固定圈检查并更换损坏部分","㎡",2560]
[9,"10号温室","外遮阳检修","遮阳网、支撑线、钢丝绳、固定圈、外遮光线路检修并更换损坏部分，天窗检修","㎡",2560]
[10,"11号温室","外遮阳检修","遮阳网、支撑线、钢丝绳、固定圈检修，天窗检修，较正外遮光立柱，更换损坏部分","㎡",2560]
[11,"其他","温室大棚排水系统井盖检修","更换20个大棚排水系统井盖","套",35]
["备注：本次投标报价最高限额为7.6万元以下，含税含发票。"]

{"sheet":"Sheet4","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet2","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}